Passive VIM Heatsink:
	Larger fin surface area, attractive design

Description:
	Our passive-internal heatsink for VIM series and Edge-V SBCs. We've extended the fins all the way to the left-side to increase surface area for passive cooling. We believe this heatsink will be popular amongst HTPC enthusiasts and those who prefer to have a silent computing/entertainment experience.

Specifications:
	Material: 6063 Aluminium
	Colour: Black
	Mounting: M2x4
	Weight: 24.0g
	Dimensions: 81.0 x 49.1 x 8.9 mm

Thermal Pad (VIM Series):
	Material: Silicone
	Colour: Blue
	Conductivity: 2.0W/mK
	Weight: 2.0g
	Dimensions: 20.0 x 20.0 x 1.6 mm

Thermal Pad (Edge-V):
	Material: Silicone
	Colour: Pink
	Conductivity: 2.0W/mK
	Weight: 1.0g
	Dimensions: 20.0 x 20.0 x 0.8 mm

Compatibility:
	VIM1
	VIM2
	VIM3
	VIM3L
	Edge-V
	DIY Case

Incompatible:
	3705 Cooling Fan
	3004 Cooling Fan
	Edge
	Captain

In the Packet:
	Passive VIM Heatsink
	Thermal Pad (Blue: VIM, Pink: Edge-V)
	x4 M2 Crosshead Screws